electronic branch

Router:

Default Gateway: 192.168.0.2

Text

Description automatically generated

Warless router:

Graphical user interface

Description automatically generated

Server:

IP address : 192.168.0.1

Subnet mask : 255.255.255.252

Graphical user interface, application

Description automatically generated

Graphical user interface

Description automatically generated

Labtop1:

Graphical user interface, application

Description automatically generated

Labtop2:

Graphical user interface, application

Description automatically generated